# Receive VCP data on raspberry PI

1. Connect Raspberry with internet
2. Dmesg | grep tty / to show interfaces / on our pi it was the ttyACM0 interface
3. sudo apt-get update / to install updates
4. sudo apt-get install screen / to intall the program “screen” for showing output of reader
5. screen /dev/ttyACM0 9600,cs8
6. Now you can scan a barcode or mifare card and you should get the output displayed