A B C D E F G H I K L M N O P R S T U V W

## K

KEY_BARCODE_BITMAP - Static variable in class com.amarula.barcodescanner.sdk.BarcodeScanner
  If chosen to get the barcode bitmap, you can get it using with this keyword.
KEY_CHANGED - Static variable in class com.amarula.barcodescanner.sdk.BarcodeScannerSymbologyTable
KEY_ENABLED - Static variable in class com.amarula.barcodescanner.sdk.BarcodeScannerSymbologyTable
KEY_FLAGS - Static variable in class com.amarula.barcodescanner.sdk.BarcodeScannerSymbologyTable
KEY_HW_LABEL - Static variable in class com.amarula.barcodescanner.sdk.BarcodeScannerSymbologyTable
KEY_LABEL - Static variable in class com.amarula.barcodescanner.sdk.BarcodeScannerSymbologyTable
KEY_MAX_LENGTH - Static variable in class com.amarula.barcodescanner.sdk.BarcodeScannerSymbologyTable
KEY_MIN_LENGTH - Static variable in class com.amarula.barcodescanner.sdk.BarcodeScannerSymbologyTable
KEY_SET_DIRECTINPUT_APPEND_ENTER_TO_TAGS - Static variable in class com.amarula.barcodescanner.sdk.BarcodeScanner
  Use this key to force the status of "Append ENTER to tags" (boolean)
KEY_SET_DIRECTINPUT_APPEND_TAB_TO_TAGS - Static variable in class com.amarula.barcodescanner.sdk.BarcodeScanner
  Use this key to force the status of "Send TAB keyevent" (boolean)
KEY_SET_DIRECTINPUT_BEEP_ON_SCAN - Static variable in class com.amarula.barcodescanner.sdk.BarcodeScanner
  Use this key to force the status of "Beep on Scan" (boolean)
KEY_SET_DIRECTINPUT_CENTERBTN_AS_SCANTRIG - Static variable in class com.amarula.barcodescanner.sdk.BarcodeScanner
  Use this key to force the status of "Center Button as Scan trigger" (boolean)
KEY_SET_DIRECTINPUT_ENABLED - Static variable in class com.amarula.barcodescanner.sdk.BarcodeScanner
  Use this key to force the status of DirectInput service (boolean)
KEY_SET_DIRECTINPUT_SCAN_MULTIPLE - Static variable in class com.amarula.barcodescanner.sdk.BarcodeScanner
  Use this key to force the status of "Scan multiple barcodes" (boolean)
KEY_SET_DIRECTINPUT_SCREEN_ON_WARM_SCANNER - Static variable in class com.amarula.barcodescanner.sdk.BarcodeScanner
  Use this key to force the status of "Screen On warm scanner" (boolean)
KEY_SET_DIRECTINPUT_TAG_PREFIX - Static variable in class com.amarula.barcodescanner.sdk.BarcodeScanner
  Use this key to force the Tag prefix String (String)
KEY_SET_DIRECTINPUT_TAG_SUFFIX - Static variable in class com.amarula.barcodescanner.sdk.BarcodeScanner
  Use this key to force the Tag suffix String (String)
KEY_SET_DIRECTINPUT_VIBRATE_ON_SCAN - Static variable in class com.amarula.barcodescanner.sdk.BarcodeScanner
  Use this key to force the status of "Vibrate on Scan" (boolean)
KEYCODE_SCAN - Static variable in class com.amarula.barcodescanner.sdk.BarcodeScanner
KEYCODE_SCAN - Static variable in class com.gen2wave.rp1600.sdk.msrocr.MSROCR

A B C D E F G H I K L M N O P R S T U V W