A B C D E F G H I K L M N O P R S T U V W

## R

read(byte[], int, int) - Method in class com.amarula.rp1600.sdk.util.SerialPort
  Read data from a serial port
read(byte[], int, int, int) - Method in class com.amarula.rp1600.sdk.util.SerialPort
  Read data from a serial port
READ_INDEXTABLE - Static variable in class com.gen2wave.rp1600.sdk.finger.OTG_KEY
READ_NOTEPAD - Static variable in class com.gen2wave.rp1600.sdk.finger.OTG_KEY
readln(byte[], int, int) - Method in class com.amarula.rp1600.sdk.util.SerialPort
  Read data from a serial port until a \n is found
REG_MODULE - Static variable in class com.gen2wave.rp1600.sdk.finger.OTG_KEY
RESPONSE - Static variable in class com.gen2wave.rp1600.sdk.finger.OTG_KEY
RETURN_ERROR - Static variable in class com.gen2wave.rp1600.sdk.finger.UsbStatus
RETURN_PINLOCK - Static variable in class com.gen2wave.rp1600.sdk.finger.UsbStatus
RETURN_SUCCESS - Static variable in class com.gen2wave.rp1600.sdk.finger.UsbStatus
RfidChangeBaudrate(int) - Method in class com.amarula.rp1600.sdk.rfid.RfidPort
RfidPort - Class in com.amarula.rp1600.sdk.rfid
  Serial Port Extension that handle RFID power supply on open/close
RfidPort() - Constructor for class com.amarula.rp1600.sdk.rfid.RfidPort
RfidPort(int, int) - Constructor for class com.amarula.rp1600.sdk.rfid.RfidPort
RP1600Constants - Class in com.amarula.rp1600.sdk
RP1600Constants() - Constructor for class com.amarula.rp1600.sdk.RP1600Constants

A B C D E F G H I K L M N O P R S T U V W