

checksum is CheckSum8 Xor over the complete telegram before the checksum itself:

http://www.scadacore.com/field-tools/programming-calculators/online-checksum-calculator/


Read FW Number
==============

Command to RFID: 50 00 00 04 54

Reply Example from RFID: 50 00 04 04 71 17 03 20 15 

Bytes "71 17 03 20" are the Firmware number.



ISO 15693
=========

Inventory
¯¯¯¯¯¯¯¯¯
Command to RFID:
>>  50 00 03 A1 06 00 00 F4
50 = start of telegram
00 03 = 3 bytes payload between command code and checksum
A1 = command code, 5.4.1 I2_INVENTORY(CMD=0xA1)
06 = Flag, 16 Slot inventory; 26 is 1 slot inventory
00 = AFI, 0x00 = no AFI used
00 = no UID will be sent with this telegram, no RFID tag will be addressed directly
F4 = checksum

Reply from RFID:
<<  50 00 08 A1 F5 25 26 9F 00 01 04 E0 75 ---success
50 = start of telegram
00 08 = 8 bytes payload between command code and checksum
A1 = command code, 5.4.1 I2_INVENTORY(CMD=0xA1)
F5 25 26 9F 00 01 04 E0 = 8 byte UID
75 = checksum


ISO 14443A
==========


Error happening: No tag in field
¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯
Command to RFID:
>>  50 00 02 22 10 26 46
50 = start of telegram
00 02 = 2 bytes payload between command code and checksum
22 = command code, 5.1.2 PICCACTIVATE(CMD=0x22)
10 = shut off antenna for 10 ms
26 = Request IDLE
46 = checksum

Reply from RFID:
<<  F0 00 01 22 E0 33 ---failure
F0 = start of telegram with error messsage
00 01 = 1 byte payload between command code and checksum
22 = command code, 5.1.2 PICCACTIVATE(CMD=0x22)
E0 = no card response within given time indicating by timeout
33 = checksum


Detects Mifare with 7 byte long UID
¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯
Command to RFID:
>>  50 00 02 22 10 26 46
pls. see example before

Reply from RFID:
<<  50 00 0B 22 44 00 08 07 04 49 69 AA 2B 2B 80 3C ---success
50 = start of telegram
00 0B = 11 bytes payload between command code and checksum
22 = command code
44 00 = ATQ (Answer To Request), contains type designation
08 = SAK (Select AcKnowledge), 
07 = 7 byte long UID folows
04 49 69 AA 2B 2B 80 = 7 byte long UID
3C = checksum


Detects Mifare with 4 byte long UID
¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯
Command to RFID:
>>  50 00 02 22 10 26 46
pls. see example before

<<  50 00 08 22 02 00 18 04 03 E7 FB 6B 10 ---success
50 = start of telegram
00 08 = 8 bytes payload between command code and checksum
22 = command code
02 00 = ATQ (Answer To Request), contains type designation
18 = SAK (Select AcKnowledge), 
04 = 4 byte long UID follows
03 E7 FB 6B = 4 byte long UID
10 = checksum


Mifare Authenticate
¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯
Command to RFID:
>>  50 00 0C 16 60 05 03 E7 FB 6B FF FF FF FF FF FF 5B
50 = start of telegram
00 0C = 12 bytes payload between command code and checksum
16 = command code
60 = authenticate with Key A, use 0x61 for Key B
05 = authenticate for block #5
03 E7 FB 6B = 4 byte long UID of card
FF FF FF FF FF FF = Key
5B = checksum

Reply from RFID:
<<  50 00 00 16 46 ---success


Mifare Read Block
¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯
Command to RFID:
>>  50 00 01 17 05 43
50 = start of telegram
00 01 = 1 byte payload between command code and checksum
17 = command code
05 = read block #5
43 = checksum

Reply from RFID:
<<  50 00 10 17 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 57
50 = start of telegram
00 10 = 17 bytes payload between command code and checksum
17 = command code
00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 = 16 Bytes of read block
57 = checksum


Mifare Write Block
¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯
Command to RFID:
>>  50 00 11 18 05 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 5C 
50 = start of telegram
00 11 = 18 bytes payload between command code and checksum
18 = command code
05 = write block #5
55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 = 16 Bytes to write to target block
5C = checksum

Reply from RFID:
<<  50 00 00 18 48 ---success



AUTOLISTCARDS
=============

Switch ON Autolistcards
¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯
Command to RFID:
>> 50 00 05 23 FF 64 00 01 00 EC
50 = start of telegram
00 05 = 5 bytes payload between command code and checksum
23 = command code, 5.1.3 AUTOLISTCARD(CMD=0x23)
FF = all supported tag types*
64 = 100 decimal, interval between tag inventory in milliseconds
00 = antenna number, 00 = all antennas
01 = when shall be sent a telegram**
00 = Reserved for Future Use, do not send other value than 0x00 except for special firmware
ED = checksum

Reply from RFID: 50 00 00 23 73 (confirmation from RFID device)


>> 50 00 05 23 FF 64 00 01 00 EC no output
>> 50 00 05 23 FF 64 02 01 00 EE output




Autoread of NTAG215

50 00 10 23 01 64 03 01 00 44 00 00 07 04 2A BB 82 1D 3E 81 F2 
50 = Start of Telegram
00 10 = 10 Bytes of p
23 = Command code, auto-list cards
01 64 03 01 00 44 00 00 
07 
04 2A BB 82 1D 3E 81 
F2 




Switch OFF Autolistcards
¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯¯
Command to RFID:
>> 50 00 05 23 FF 00 01 01 00 89
50 = start of telegram
00 05 = 5 bytes payload between command code and checksum
23 = command code, 5.1.3 AUTOLISTCARD(CMD=0x23)
FF = all supported tag types*
00 = interval between tag inventory, 00 switches OFF
01 = antenna number
01 = when shall be sent a telegram**
00 = Reserved for Future Use, do not send other value than 0x00 except for special firmware
89 = checksum

Reply from RFID: 50 00 00 23 73 (confirmation from RFID device)


* Select Tag Type
0x01: ISO14443 A card only
0x04: ISO15693 Only
0x05: ISO15693 + ISO14443 A
0x00, 0xFF: All card type the module supported

**
0x01 = NOTICE when a tag enters the field
0x02 = NOTICE when a tag leaves the field
0x03 = NOTICE when a tag enters and leaves the field
0x04 = NOTICE continuously as long as the tag is in field, notification interval is the inventory interval